Altium Designer Pick and Place Locations
K:\Work\KNIVD\ELLO\1A\hardware\project outputs\Pick Place for PCB.txt

========================================================================================================================
File Design Information:

Date:       28/02/21
Time:       09:55
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                Layer    Footprint                     Center-X(mm) Center-Y(mm) Rotation Description                                                                                                                
R4         330R                   TopLayer RES1016-660X250-1206          25.5000      -20.5000     270      Resistor                                                                                                                   
D1         1N4148                 TopLayer DO-35_/_1206+                 51.0000      -23.0000     180      Diode                                                                                                                      
UALT1      PIC32MX170F256B-50I/SO TopLayer SOIC127P1032X265-28N          17.0000      -26.5000     180      "32-bit Microcontrollers (up to 128 KB Flash and 32 KB SRAM) with Audio and Graphics Interfaces, USB, and Advanced Analog" 
R3         10k                    TopLayer RES1016-660X250-1206          29.0000      -33.0000     270      Resistor                                                                                                                   
U1         PIC32MX170F256B-50I/SP TopLayer DIP28-300                     13.3000      -32.5000     180      "32-bit Microcontrollers (up to 128 KB Flash and 32 KB SRAM) with Audio and Graphics Interfaces, USB, and Advanced Analog" 
SW1        OS102011MA1QN1         TopLayer OS102011MA1QN1                12.0000      -57.5000     360      Switch                                                                                                                     
SPK1       MCKP12-G185B-3709      TopLayer BUZZER65/120                  24.2500      -44.5000     270      Speaker/Buzzer                                                                                                             
R2         330R                   TopLayer RES1016-660X250-1206          10.0000      -53.0000     180      Resistor                                                                                                                   
OSC1       MXO45HS-3C-20M000000   TopLayer OSC_13.2x13.2_/_70x50         22.0000      -7.2500      360      "Low-Power CMOS Oscillator"                                                                                                
LED1       MV5437                 TopLayer LED_5MM_RED_GREEN_1AR-2CC-3AG 23.5000      -56.5000     0        "Bicolor Red/Green  LED 1 Anode Red 2 Com Cathode 3 Anode Green"                                                           
JP1        DIL6-M                 TopLayer SAMTEC_MTLW-103-07-L-D-250    41.7500      -24.7500     180      "2.54mm square pin header/jumper"                                                                                          
J5         XM7D-0512              TopLayer WURTH_651005136521            10.5500      -4.6750      180      "USB mini/micro, 5 Position Receptacle"                                                                                    
J4         DM1AA-SF-PEJ           TopLayer DM1AA-SF-PEJ                  46.7500      -42.0000     360      "SD card connector"                                                                                                        
J3         DIL10-F                TopLayer 2011-2X05S                    66.0000      -45.5000     270      "Dual row, 10-way connector"                                                                                               
J2         999-H15-PS2L571        TopLayer 999-H15-PS2L571               45.7500      -12.5665     180      "D-sub 15HD over two PS/2 connector"                                                                                       
C7         10u                    TopLayer CAPRR508-350X500X500-1206     4.0000       -9.5000      360      Capacitor                                                                                                                  
C6         10u                    TopLayer CAPRR508-350X500X500-1206     4.0000       -24.0000     180      Capacitor                                                                                                                  
C5         10u                    TopLayer CAPRR508-350X500X500-1206     51.0000      -26.0000     180      Capacitor                                                                                                                  
C4         100n                   TopLayer CAPRR508-350X500X500-1206     11.5000      -11.0000     180      Capacitor                                                                                                                  
C3         10u                    TopLayer CAPRR508-350X500X500-1206     25.5000      -33.0000     90       Capacitor                                                                                                                  
C2         10u                    TopLayer CAPRR508-350X500X500-1206     4.0000       -28.0000     360      Capacitor                                                                                                                  
C1         100n                   TopLayer CAPRR508-350X500X500-1206     4.0000       -49.0000     360      Capacitor                                                                                                                  
R1         10k                    TopLayer RES1016-660X250-1206          6.2500       -41.0000     270      Resistor                                                                                                                   
J1         SIL5-M                 TopLayer 2011-1X05S                    3.2500       -38.0000     90       "Single row, 5-way connector"                                                                                              
U2         MCP1826-3302E/AT       TopLayer TO220-5                       4.2500       -16.7500     90       "1000 mA, Low Voltage, Low Quiescent Current  LDO Regulator"                                                               
UALT2      MCP1826T-3302E/DC      TopLayer SOT127P700X180-6N             4.1750       -16.6250     180      "1000 mA, Low Voltage, Low Quiescent Current  LDO Regulator"                                                               
